FAST ** = 0o

FAST ** = 45o

Exp. **= 0o

Exp. ** = 45o

FAST ** = 0o

FAST ** = 45o

Exp. **= 0o

Exp. ** = 45o

The pitch angle change in the cyclic pitch control is given by the following expression:



Here, *ψ* is the azimuth angle, *ξ* is the phase angle of the pitch angle *θ* with respect to the azimuth angle *ψ*, *a* is the pitch angle amplitude, and *b* is the average pitch angle.

